(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "PermaBread")
		(date "2025-03-26")
		(rev "1")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "../../Downloads/bread/")
		)
	)
	(net 0 "")
	(gr_arc
		(start 97.86 138)
		(mid 95.73868 137.12132)
		(end 94.86 135)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.78 138)
		(end 97.86 138)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 199.78 135)
		(mid 198.90132 137.12132)
		(end 196.78 138)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 99.06 134.62)
		(end 100.41 134.62)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.86 135)
		(end 94.86 86)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 195.58 134.62)
		(end 196.93 134.62)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 195.58 86.36)
		(end 196.93 86.36)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.78 86)
		(end 199.78 135)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 94.86 86)
		(mid 95.73868 83.87868)
		(end 97.86 83)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 97.86 83)
		(end 196.78 83)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 196.78 83)
		(mid 198.90132 83.87868)
		(end 199.78 86)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 99.06 86.36)
		(end 100.41 86.36)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "PermaBread V.1"
		(at 104.14 111.76 0)
		(layer "F.Cu")
	)
	(embedded_fonts no)
)
